**Tata Concept S**

**Technical Specifications**

|  |  |
| --- | --- |
| Engine | 1.3 L SDE Euro-5 |
|  |
| Max. Engine Output  | 70 kW @ 4000 rpm |
|  |
| Max. Torque  | 200 Nm @ 1500 rpm |
|  |
| Steering | Hydraulic Power Assisted |
|  |
| Gearbox | 5 + 1 Reverse Transaxle |
|  |
| Length x Width x Height (mm) | 3795 x 1695 x 1550  |
|  |
| Wheelbase (mm) | 2470 |
|  |
| Tyre Size | 205/40 R17 |
|  |
| Max. Speed (km/h) | 160 |
|  |
| Luggage Space (litres) | 232  |

**Standard / Optional Features**

**Safety**

* Airbags – passenger, side
* ABS with EBD
* Remote operated central locking with transponder in key
* Immobiliser
* Front and rear fog lamps
* Rear windscreen wash and wipe
* Rear glass demisting
* Light intensity adjustment on instrument cluster

**Comfort**

* Four-way seat adjustment
* Tilt-adjust Steering
* Power windows
* Lumbar support
* Electrically operated ORVM
* 60:40 rear seat split
* Socket for mobile charger
* Fully automatic temperature control
* Touch screen music system
* Navigation system